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[bookmark: _Toc42488098]ANNEX II + III:	 TECHNICAL SPECIFICATIONS + TECHNICAL OFFER
Contract title: Procurement of Equipment for Fire and Rescue Units in the Republic of Srpska within the INEREP Project
Lot 2: Supply of Rescue Boat with Outboard Motor and Trailer	
Publication reference: 25.02-810.2-74/26


Columns 1-2 should be completed by the contracting authority
Columns 3-4 should be completed by the tenderer
Column 5 is reserved for the evaluation committee 
Annex III - the contractor's technical offer
The tenderers are requested to complete the template on the next pages: 
· Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer), 
· Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)  
· Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation
The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.
The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offered specifications.

The subject of Lot 2 is the supply and delivery of 1 rescue boat with accompanying equipment, consisting of 1 polyethylene rescue boat, 1 outboard motor and 1 trailer 
for boat transport.

The rescue boat shall be used for rescue and civil protection interventions on water, including flood response, evacuation support, rescue operations and other 
emergency interventions requiring safe transport and operation on water.

1. General requirements
1.1 The tenderer shall ensure that the functions and features of the offered rescue boat, outboard motor and trailer meet all minimum requirements set out in these 
Technical Specifications.
1.2 All specification details listed in these Technical Specifications represent minimum requirements, unless stated otherwise. Any improvements or additional features
offered by the tenderer shall be clearly identified in the technical offer.
1.3 The offered rescue boat, outboard motor and trailer must be new, unused and fully compliant with the required technical specifications and applicable standards.
1.4 The supplies shall include the rescue boat, outboard motor, trailer for boat transport, mounting of the motor on the boat, initial (zero) service of the outboard motor, 
all required technical documentation, catalogues or technical sheets, certificates, warranty documents, user manuals, service documentation, maintenance plan and all 
other documents required for proper delivery, registration, obtaining of the navigation permit, use, maintenance and acceptance.
1.5 The tenderer shall clearly indicate the offered make, model, type and configuration of the rescue boat, outboard motor and trailer.
1.6 The tenderer shall submit catalogues or technical sheets issued by the manufacturer or authorised distributor, clearly showing the offered model and all requested 
technical characteristics.
1.7 The documentation supplied shall clearly indicate, highlight or mark the models offered and the options included, if any, so that the evaluation committee can 
identify the exact configuration offered.
1.8 Offers that do not permit the precise identification of the offered models, configuration and technical characteristics may be rejected by the evaluation committee.
1.9 Where these Technical Specifications refer to a particular standard, make, source, process, trademark, patent, type or origin, the words “or equivalent” shall be 
deemed to apply. Any equivalent solution must meet or exceed the required functional, technical, safety and performance requirements. The tenderer shall provide 
documentary evidence demonstrating equivalence. This provision shall not permit any reduction of the required quantities, minimum performance levels, capacities, 
dimensions or other expressly stated mandatory requirements.


2. Service and maintenance requirements
2.1 The tenderer shall submit a certified statement confirming that authorised warranty and after-sales service for the offered outboard motor is available in Bosnia 
and Herzegovina or will be made available no later than the date of delivery, at no additional cost to the contracting authority.
2.2 The statement shall include the name and address of the authorised service provider or providers. Where the service will be established or contracted after 
submission of the tender, the tenderer shall provide evidence of the relevant commitment or arrangement no later than the date of delivery. 
2.3 The tenderer must 
submit a regular maintenance plan for the offered outboard motor, issued by the manufacturer or authorised service provider of the offered 
outboard motor.
2.4 The tender must include mounting of the outboard motor on the boat and initial service of the motor.
3. Warranty conditions
3.1 Warranty shall apply in accordance with Article 32 of the General Conditions, the Special Conditions and these Technical Specifications.
3.2 Warranty for the rescue boat, outboard motor and trailer shall be minimum 12 months from the date of provisional acceptance..
3.3 The contractor shall be responsible for maintenance and repair of the supplies within the warranty period, in accordance with the warranty conditions and the 
contract.
3.4 The contractor shall guarantee the proper operation of the supplied rescue boat, outboard motor and trailer. In the event of failure during the warranty period, the 
contractor shall restore proper operation or, where repair is not possible, replace the defective item with equivalent supplies at its own cost.
4. Delivery, registration and navigation permit documentation
4.1 For Lot 2, the maximum period of implementation shall be 280 calendar days, starting from the date on which the contract is signed by the last party. The delivery 
period shall be 250 calendar days. The period of implementation shall end on the date of issuance of the Provisional Acceptance Certificate. The certificate shall be 
issued or refused within 30 calendar days of receipt of the contractor’s complete application for provisional acceptance.
4.2 The delivery location: The rescue boat, outboard motor and trailer shall be delivered DDP to the Civil Protection Administration of the Republic of Srpska, 
Spasovdanska 3, 71123 East Sarajevo, Republic of Srpska, Bosnia and Herzegovina.
4.3 Upon delivery of the rescue boat, outboard motor and trailer, the contractor must provide all documentation necessary for registration, obtaining the navigation 
permit, legal use and provisional acceptance, where applicable, in Bosnia and Herzegovina.
4.4 The documentation required for registration and obtaining the navigation permit shall include the invoice, certificates and technical documentation for the rescue 
boat, outboard motor and trailer, homologation or conformity documents where applicable, evidence of completion of the initial (zero) service of the outboard motor, 
and the customs declaration where applicable.
4.5 A customs declaration shall be provided where applicable under the customs rules governing the importation of the supplied rescue boat, outboard motor or trailer.
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	1
	POLYETHYLENE BOAT 
Quantity: 1 piece
	
	
	

	1.1	
	Length: minimum 435 cm.
	
	
	

	1.2
	Width: minimum 170 cm.
	
	
	

	1.3
	Weight: maximum 190 kg.
	 
	
	

	1.4
	Carrying capacity: CE category “C” – 8 persons; category “D” – 10 persons.
	
	
	

	1.5
	Permitted weight: C 980 kg / D 980 kg.
	
	
	

	1.6
	Recommended engine power: 30 HP, long shaft.
	
	
	

	1.7
	Category: “C”.
	
	
	

	1.8
	Construction: polyethylene moulded in one piece.
	
	
	

	1.9
	Colour: grey or red.
	
	
	

	1.10
	Condition: new and unused boat.
	
	
	

	1.11
	Warranty: minimum 12 months.
	
	
	

	1.12
	Catalogue or technical sheet of the offered boat.
	
	
	

	2
	OUTBOARD MOTOR FOR BOAT 
Quantity: 1 piece
	
	
	

	2.1
	Engine type: 4-stroke.
	
	
	

	2.2
	Fuel: petrol.
	
	
	

	2.3
	Engine capacity: DELETED
	
	
	

	2.4
	Number of cylinders / configuration: in-line 3 cylinders.
	
	
	

	2.5
	SOHC.
	
	
	

	2.6
	Propeller shaft power: minimum 22.1 kW at 5,500 rpm.
	
	
	

	2.7
	Lubrication system: oil pump.
	
	
	

	2.8
	Fuel supply: Electronic Fuel Injection (EFI) or technically equivalent electronic fuel-injection system.
	
	
	

	2.9
	Gear ratio: minimum 2.00 (26/13).
	
	
	

	2.10
	Recommended transom height: 508 mm.
	
	
	

	2.11
	Weight with propeller: maximum 98 kg.
	
	
	

	2.12
	Propeller protection: no.
	
	
	

	2.13
	Fuel tank: separate, 25 l.
	
	
	

	2.14
	Engine oil capacity: maximum 1.7 l, including oil filter replacement.
	
	
	

	2.15
	Steering: manual.
	
	
	

	2.16
	Colour: grey, black, red or a combination of these colours.
	
	
	

	2.17
	Condition: new and unused motor.
	
	
	

	2.18
	Warranty: minimum 12 months.
	
	
	

	2.19
	The offer must include mounting of the motor on the boat and initial service of the motor.
	
	
	

	2.20
	Catalogue or technical sheet of the offered outboard motor.
	
	
	

	3
	TRAILER FOR BOAT TRANSPORT 
Quantity: 1 piece
	
	
	

	3.1
	Total trailer mass: 750 kg.
	
	
	

	3.2
	Empty trailer mass: maximum 150 kg.
	
	
	

	3.3
	Permitted load capacity: minimum 600 kg.
	
	
	

	3.4
	External trailer length: minimum 680 cm.
	
	
	

	3.5
	Total usable length: minimum 580 cm.
	
	
	

	3.6
	External width: maximum 180 cm.
	
	
	

	3.7
	Wheels: 155/70 R13.
	
	
	

	3.8
	Axle load capacity: 1 x 750 kg.
	
	
	

	3.9
	Jockey wheel with clamps.
	
	
	

	3.10
	Coupling/drawbar: must be adapted to a standard Euro tow hook.
	
	
	

	3.11
	Installation: 12 V, light signalling through a plug compatible with the standard connector on the towing vehicle.
	
	
	

	3.12
	Category: O1 - trailer vehicle.
	
	
	

	3.13
	Colour: grey or white.
	
	
	

	3.14
	Condition: new and unused trailer.
	
	
	

	3.15
	Warranty: minimum 12 months.
	
	
	

	3.16
	The trailer must be ready for registration with all accompanying documentation.
	
	
	

	3.17
	Catalogue or technical sheet of the offered trailer for boat transport.
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